5 Channel EGT Amp

Requirements

1. Amplify K-type Thermocouple to usable analog voltage
2. Read voltage on all channels with attached Thermocouple
3. Send thermocouple reading on canbus
4. Use compound ID for each individual channel

Use Case

1. If no thermocouple attached to channel send default value
2. Can bus failure, reset chip